waits for ly 141
enables lyc
enables m1irq
sets lyc to 143
interrupt enable

on int
jumps to 0x1000
does a bunch of nops
reads IF
outputs value of IF&3

lycint142_m1irq_1.gb should output 0
lycint142_m1irq_2.gb should output 3
