waits for mode3
enables mode 2 int
waits for int

on int jumps to 0x1000
nops til late mode0
disables mode2 irq
reads IF
outputs value of IF&3

disable_1.gbc should output 0
disable_2.gbc should output 2
