waits for mode2
enables mode 0 int
waits for int

on int jumps to 0x1000
disables mode0 irq
nops til late next mode0
enables mode0 irq
reads IF
outputs value of IF&3

late_enable_1.gbc should output 2
late_enable_2.gbc should output 0
