waits until ly=3
sets lyc to 5
enables lyc int
waits for int

on int:
jumps to 0x1000
nops til next ly
sets lyc to 6
sets STAT to 0
sets IF to 0
sets STAT to 0x40
reads IF
outputs value of IF&3

ff41_reenable_2.gb should output 2
