waits for ly 150
enables lyc
sets lyc to 152
interrupt enable

on int
jumps to 0x1000
does a bunch of nops
enables mode1 irq
reads IF
outputs value of IF&3

m1irq_late_enable_1.gbc should output 2
m1irq_late_enable_2.gbc should output 0
