waits for mode2
enables mode 0 int
waits for int

on int jumps to 0x1000
lots of nops
reads stat
outputs value of stat&3

DMG-01 / CGB-001:
m0int_m3stat_1.gb should output 3
m0int_m3stat_2.gb should output 0