waits until ly=3
sets lyc to 5
enables lyc int
waits for int

on int:
jumps to 0x1000
lots of nops
reads stat
outputs value of stat&3

DMG-08 / CGB:
lycint_m0stat_1.gb should output 0
lycint_m0stat_2.gb should output 2
