waits until ly=91
sets lyc to 93
enables lyc int
waits for int

on int:
sets lyc to 94
jumps to 0x1000
lots of nops
disables display
reads IF
outputs value of IF&3

ff40_disable_1.gb should output 0
ff40_disable_2.gb should output 2
